**SKETCH FOR LED\_FLASHER**

void setup()

{

pinMode(13, OUTPUT);

}

void loop()

{

digitalWrite(13, HIGH);

delay(500); \\the LED will remain switched on, for 500 milliseconds\\

digitalWrite(13, LOW);

delay(500); \\the LED will remain switched off, for 500 milliseconds\\

}